### 1.1.1 Front Panel

Figure1-2 Front Panel of LS2-24GT4SFP-P

Note

indicates PoE+ port, which is compliant with IEEE 802.3af and IEEE 802.3at.

Table1-1 Front Panel Description of LS2-24GT4SFP-P

No. | Silkscreen | Component | Description
1 | SYS | System status LED | For details about the LED status, see 1.1.3 LED.
2 | LED MODE | Port LED switch | l LED switch toggled to left (Mode 1): the port LED status indicates the status of traffic transmission. l LED switch toggled to right (Mode 2): The port LED status indicates the PoE status.
3 | RESET | Reset button | l Press and hold the button for less than 2s: Restart the switch. l Press and hold the button for more than 5s: Press and hold the button for more than 5s until the system status LED starts blinking to restore factory settings and restart the switch. l Press and hold for 2s to 5s: No action is triggered.
4 | 1-24 | 10/100/1000Base-T Ethernet port status LED | For details about the LED status, see 1.1.3 LED.
5 | 1-24 | 10/100/1000Base-T Ethernet port | 24 x 10/100/1000BASE-T ports, with ports 1-24 supporting PoE/PoE+.
6 | 25-28 | SFP port status LED | For details about the LED status, see 1.1.3 LED.
7 | 25-28 (1G) | 1GE SFP port | 4 x 1GE SFP Port
8 | / | Nameplate | The nameplate is located at the bottom of the device.