## 1.3 Cooling

The LS2-24GT4SFP-P switch adopts the front-to-rear airflow + left-to-rear airflow design to ensure that the switch works properly in the specified environment. Maintain a minimum clearance of 100 mm (3.94 in.) around the switch to ensure proper ventilation. You are advised to dust the switch at an interval of three months to avoid blocking the ventilation openings.

Figure1-4 Airflow Direction