### 3.3.1 Installing the Switch in a Rack

The switch follows the EIA standard dimensions and can be installed in the 19-inch rack.

(1) Attach the mounting brackets to the switch with the supplied screws.

Figure3-1 Securing Rack-Mount Brackets

(2) Use the supplied M6 screws and cage nuts to securely attach the mounting brackets to the rack.

Figure3-2 Securing Rack-Mount Brackets to the Rack (1)

Figure3-3 Securing Rack-Mount Brackets to the Rack (2)